MODULE Linux arm 7CCF8FE15BFFE067000721F229100BC30 sensorservice
FILE 0 /builds/slave/b2g_m-cen_emu-kk_ntly-00000000/build/frameworks/native/include/binder/BinderService.h
FILE 1 /builds/slave/b2g_m-cen_emu-kk_ntly-00000000/build/frameworks/native/services/sensorservice/main_sensorservice.cpp
FILE 2 /builds/slave/b2g_m-cen_emu-kk_ntly-00000000/build/system/core/include/utils/StrongPointer.h
FUNC 764 8c 0 android::BinderService<android::SensorService>::publish(bool)
764 4 37 0
768 2 37 0
76a 6 38 0
770 2 88 2
772 1c 41 0
78e e 128 2
79c 2 129 2
79e 10 130 2
7ae a 41 0
7b8 2 142 2
7ba 2 41 0
7bc 2 142 2
7be e 143 2
7cc 6 41 0
7d2 4 142 2
7d6 e 143 2
7e4 c 42 0
FUNC 7f0 32 0 android::BinderService<android::SensorService>::joinThreadPool()
7f0 2 54 0
7f2 6 55 0
7f8 6 56 0
7fe 6 57 0
804 a 58 0
80e 4 142 2
812 e 143 2
820 2 59 0
FUNC 822 10 0 main
822 2 22 1
824 6 45 0
82a 4 46 0
82e 4 25 1
STACK CFI INIT 764 8c .cfa: sp 0 + .ra: lr 0 +
STACK CFI 768 .cfa: sp 40 + .ra: .cfa -4 + ^ r0: .cfa -40 + ^ r1: .cfa -36 + ^ r2: .cfa -32 + ^ r3: .cfa -28 + ^ r4: .cfa -24 + ^ r5: .cfa -20 + ^ r6: .cfa -16 + ^ r7: .cfa -12 + ^ r8: .cfa -8 + ^
STACK CFI INIT 7f0 32 .cfa: sp 0 + .ra: lr 0 +
STACK CFI 7f2 .cfa: sp 16 + .ra: .cfa -4 + ^ r0: .cfa -16 + ^ r1: .cfa -12 + ^ r2: .cfa -8 + ^
STACK CFI INIT 822 10 .cfa: sp 0 + .ra: lr 0 +
STACK CFI 824 .cfa: sp 8 + .ra: .cfa -4 + ^ r3: .cfa -8 + ^
